**Font Name PCL 5 Escape Sequence Print Example**

Troy E-13B <esc>(0Q<esc>(s1p12.0v0s0b0T 1234567890ABCD

<esc>(0Q<esc>(s0p8.00h8.8v0s0b0T

Troy CMC-7 <esc>(0Q<esc>(s1p12.0v0s0b1T 1234567890ABCD

<esc>(0Q<esc>(s0p8.00h8.8v0s0b1T

Troy ECF <esc>(3Q<esc>(s1p<height>0v0s0b0T 1234567890 BCDEFGHIJA$\*,

<esc>(3Q<esc>(s1p18v0s0b0T

Troy LCF <esc>(1Q<esc>(s0p5.01h16.0v0s0b0T 1234567890 $C%&\*,

Troy SCF <esc>(2Q<esc>(s0p6.00h22.0v0s0b0T 1234567890 $%&\*,

Troy Micro Font <esc>(10U<esc>(s0p80h.8v0s33b0T 1234567890ABCD! 1234567890ABCD! 1234567890ABCD! 1234567890ABCD! 1234567890ABCD! 1234567890ABCD! 1234567890ABCD! 1234567890ABCD!

Troy Helvetica (Rev) <esc>(9U<esc>(s1p<height>v0s33b24580T 1234567890 ABCDEFGHIJKLMnopqrstuvwxyz

Troy OCR-A <esc>(0O<esc>(s1p<height>v0s0b104T 1234567890 ABCDEFGHIJKLMnopqrstuvwxyz

Troy OCR-B <esc>(1O<esc>(s1p<height>v0s0b110T 1234567890 ABCDEFGHIJKLMnopqrstuvwxyz

1234567890 .#$%&,

Troy Security <esc>(4Q<esc>(s1p<height>v0s0b0T

**Notes**

<esc> represents the non-printable escape character (Ascii 27/Hex 1B).

<height> represents the point-size value of the scalable font. Value is represented in points .1/72inch increments.

Multiple PCL 5 font calls are shown for some fonts. Refer to the printer documentation to verify which calls your specific model supports.

These fonts may not be included with your TROY Security Printing Solution. Refer to the printer documents for details. If these fonts are not included, alternate printer-resident fonts will be printed in place of them; this is normal. If you would like to add these fonts to your printer-resident font collection, contact TROY Group, Inc. at 800-633-2266.